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ClarkDietrich® Low-Embodied Carbon (LEC) Cold-Formed Steel Framing
Section 054000 – Cold-Formed Metal Framing
NOTE:
Turn on hidden text to view important non-printing notes by selecting Show/Hide (¶) in the Paragraph Group, or by using the Ctrl+* keyboard shortcut.
Note to Specifier: The language provided herein is intended to be supplementary to Division 05 Cold-Formed Metal Framing Sections. It contains the necessary language for the specification of Low-Embodied Carbon (LEC) Cold-Formed Steel Framing products only. Coordinate with Related Requirements in applicable Division 01 Sections.
PART 1 -  GENERAL
Retain Paragraph below to cross-reference requirements Contractor might expect to find in this Section but are specified in other Sections. These may include “Section 013329 – Sustainable Design Reporting,” “Section 013563 – Sustainability Certification Project Requirements,” “Section 013566 – Sustainability Certification Project Procedures,” “Section 018113 – Sustainable Design Requirements” or related Sections.
1.1 SUMMARY
A. Related Requirements:
1. <Insert Section Number and Title>.
1.2 ACTION SUBMITTALS
A. Sustainable Design Submittals:
1. Low-Embodied Carbon (LEC) Environmental Product Declaration (EPD): For applicable products specified in Part 2.
a. Product-Specific Type III Environmental Product Declaration (EPD): Third-party verified, in conformance with ISO 14025 and EN 15804.
1) Global Warming Potential (GWP) values in kg CO₂e per declared unit.
PART 2 -  PRODUCTS
2.1 MANUFACTURERS
Retain "Basis-of-Design Product" Paragraph below to require a specific product or a comparable product from manufacturer listed.
A. Basis-of-Design Product: Subject to compliance with requirements, provide cold-formed steel framing products by ClarkDietrich; as specified in other Part 2 articles or comparable products by a current member of the SFIA.
2.2 COLD-FORMED STEEL FRAMING MATERIALS
A. Low-Embodied Carbon (LEC) Requirements:
1. Global Warming Potential (GWP) Thresholds: For [Exterior cold-formed steel framing] [Floor framing] [Steel framing connectors] complying with ASTM A1003/A1003M.
Maximum 2,228 kg CO₂e/ton cradle-to-gate is a recommended threshold determined by the U.S. General Services Administration.
a. Maximum 2,228 kg CO₂e/ton cradle-to-gate.
[bookmark: _Hlk176259066][bookmark: _Hlk179889201]Retain first option in "Framing Members, General" Paragraph below for 2015 IBC; second option for 2018, 2021, or 2024 IBC.
B. [bookmark: _Hlk160517919][bookmark: _Hlk172721102][bookmark: _Hlk186099227]Framing Members, General: Comply with [AISI S200 and ASTM C955, Section 8] [AISI S240] for conditions indicated.
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