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This Shortform Specification is intended to be used only as a “Guide” for adding product information to existing full-length Specification Sections. The user accepts responsibility for all Project Specifications. ClarkDietrich bears no responsibility for errors or omissions in any portions of the Project.
ClarkDietrich® Interior Finishing
SECTION 092900
GYPSUM BOARD
NOTE:
Turn on hidden text to view important non-printing notes by selecting Show/Hide (¶) in the Paragraph Group, or by using the Ctrl+* keyboard shortcut.
PART 1 -  GENERAL
1.1 SUMMARY
A. Section Includes:
1. Trim accessories.
2. Joint treatment materials.
Retain "Related Requirements" Paragraph below to cross-reference requirements Contractor may expect to find in this Section but are specified elsewhere. These may include but are not limited to: Section 061600 “Sheathing,” Section 092116 “Gypsum Board Assemblies,” Section 092116.23 “Gypsum Board Shaft Wall Assemblies,” Section 092216 “Non-Structural Metal Framing,” Section 092613 “Gypsum Veneer Plastering,” Section 093013 “Ceramic Tiling,” or related Sections.
B. Related Requirements:
1. <Insert Section Number and Title>.
PART 2 -  PRODUCTS
2.1 TRIM ACCESSORIES
A. Interior Trim: ASTM C1047.
1. Material: [Galvanized steel sheet, rolled zinc, vinyl, PVC-based composite, or paper-faced galvanized-steel sheet] [Galvanized steel sheet or rolled zinc] [Vinyl] [PVC-based composite] [Paper-faced galvanized-steel sheet].
2. Shapes:
a. Cornerbead.
1) [bookmark: _Hlk532885198]Product: ClarkDietrich; [103 Deluxe Corner Bead] [Paper-Faced Corner Bead] [Quicksilver Corner Bead] [Strait-Flex Original] [Vinyl Corner Bead] [West Coast Corner Bead] or comparable product.
b. Bullnose bead.
1) Product: ClarkDietrich; [Bullnose Corner Bead] [Paper-Faced Bullnose Tape-On Cornerbead] [Vinyl Bullnose Corner Bead] or comparable product.
c. LC-Bead: J- or U-shaped; joint compound is applied to exposed long flange.
1) [bookmark: _Hlk532885318]Product: ClarkDietrich; [Metal U-Trim #200-A] [Muddable J-Bead] [Rip-Bead Muddable J-Bead] or comparable product.
d. L-Bead: L-shaped; joint compound is applied to exposed long flange.
1) [bookmark: _Hlk532885403]Product: ClarkDietrich; [Metal L-Trim #200-B] [Rip-Bead Flat L-Bead] [Rip-Bead L-Bead] [Strait-Flex L-Bead] [Vinyl L-Bead] or comparable product.
e. U-Bead: J-shaped; does not require joint compound.
1) [bookmark: _Hlk532885430][bookmark: _Hlk535317046]Product: ClarkDietrich; [Metal J-Trim M400 Series] [Vinyl J-Bead] or comparable product.
f. Control Joint.
1) [bookmark: _Hlk71532313][bookmark: _Hlk532885478]Product: ClarkDietrich; [093 Control Joint] [093 Vinyl Control Joint] or comparable product.
g. Curved-Edge Cornerbead: With notched flanges that conform to curves and arches.
1) [bookmark: _Hlk71532364]Product: ClarkDietrich; [PRO-90 Archway] [PRO-Bull 3/4" Archway] [Strait-Flex Arch-Flex] [Strait-Flex Arch Stick] or comparable product.
3. Flexible Corner Types:
a. Wall Corner Trim (Stick Corner Beads):
1) Product: ClarkDietrich; [Strait-Flex OS-400] [Strait-Flex Big-Stick] [Strait-Flex Wet-Stick] or comparable product.
b. Inside Corner:
1) Product: ClarkDietrich; [Strait-Flex Original] [Strait-Flex IS-300] [Strait-Flex Pro-Flex 300] or comparable product.
c. Edge Trim:
1) Product: ClarkDietrich; Strait-Flex Edge-Tape or comparable product.
d. Vaults/Soffits:
1) ClarkDietrich; [Strait-Flex Gold] [Strait-Flex Pro-Flex 300] or comparable product.
2.2 JOINT TREATMENT MATERIALS
A. General: Comply with ASTM C475/C475M.
B. Joint Tape:
1. Interior Gypsum Board: Paper-based; general use.
a. [bookmark: _Hlk6469522]Product:  ClarkDietrich; Strait-Flex Butt-Tape or comparable product.
2. Tile Backing Panels: Composite; for use with fiber cement board, green board, mold-resistant board, or water-resistant board in wet areas.
a. [bookmark: _Hlk6469565]Product: ClarkDietrich; Strait-Flex Tile-Tape or comparable product.
PART 3 -  EXECUTION
3.1 INSTALLATION OF TRIM ACCESSORIES
A. General: Install in accordance with ASTM C840 and manufacturer’s written instructions.
B. Control Joints: Install [at locations indicated on Drawings] [in accordance with ASTM C840 and specific locations approved by Architect].
C. Interior Trim: Install in locations as follows:
Cornerbead: At outside corners [unless otherwise indicated] <Insert requirements>.
Bullnose Bead: [At outside corners] [As indicated on Drawings] <Insert requirements>.
LC-Bead: [At exposed panel edges] [As indicated on Drawings] <Insert requirements>.
L-Bead: [As indicated on Drawings] <Insert requirements>.
U-Bead: [At exposed panel edges] [As indicated on Drawings] <Insert requirements>.
Curved-Edge Cornerbead: [At curved openings] [As indicated on Drawings] <Insert requirements>.
3.2 APPLYING JOINT TREATMENT MATERIALS
A. General: Install in accordance with ASTM C840 and manufacturer’s written instructions.
B. Apply joint tape at gypsum board and tile-backing panel joint locations unless otherwise indicated.
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